DAILY ASSESSMENT FORMAT

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Date: | | 06 JUNE 2020 | | Name: | RACHANA C HULIKATTI |
| Course: | | DIGITAL DESIGN USING HDL | | USN: | 4AL17EC108 |
| Topic: | | Verilog HDL Basics by Intel  Verilog Test bench code to  Verify the design under the test (DUT) | | Semester  & Section: | 6TH B |
|  |  | |

|  |
| --- |
| FORENOON SESSION DETAILS |
|  |

|  |
| --- |
| Report –      FPGA Basics: Architecture, Applications and Uses:     * Abasic FPGA architecture (Figure 1) consists of thousands of fundamental elements called configurable logic blocks (CLBs) surrounded by a system of programmable interconnects, called a fabric, that routes signals between CLBs. Input/output (I/O) blocks interface between the FPGA and external devices. Dependingonthemanufacturer, the CLBmayalsobereferredto as alogicblock(LB), a logic   element (LE) or a logic cell (LC).    Application:    Manyapplicationsrelyontheparallelexecutionofidenticaloperations;theabilityto configure the FPGA’s CLBs into hundreds or thousands of identical processing blocks has applications in image processing, artificial intelligence (AI), data center hardware accelerators, enterprise networking and automotive advanced driver assistance systems (ADAS).Manyoftheseapplicationareasarechangingveryquicklyasrequirementsevolveand newprotocols andstandardsareadopted. FPGAsenablemanufacturerstoimplement systems that can be updated when necessary. A good example of FPGA use is high-speed search: Microsoft is using FPGAs in its data |

|  |
| --- |
| centerstorun Bingsearchalgorithms. The FPGAcanchangetosupportnewalgorithms astheyare created. If needschange, thedesigncanberepurposedtorunsimulationor modelingroutinesin an HPC application. Thisflexibilityisdifficultorimpossibleto achieve with an ASIC. Other FPGA uses include aerospace and defense, medical electronics, digital television, consumer electronics, industrial motor control, scientific instruments, cybersecurity systems and wireless communications.  Verilog HDL Basics by Intel:  Verilog is a HARDWARE DESCRIPTION LANGUAGE (HDL). It is a language used for describingadigitalsystem likeanetworkswitchor amicroprocessorora memory or a flip−flop. It means, by using a HDL we can describe any digital hardware at any level. Designs, which are described in HDL are independent of technology, very easy for designing and debugging, and are normally more useful than schematics, particularly for largecircuits.  Behavioral level ,Register-transfer level ,Gate level ,Lexical Tokens ,Numbers ,Identifiers ,Operators ,Data Types , Operators , Operands , Modules |

|  |
| --- |
| Verilog Test bench code to verify the design under test (DUT):  TASK:  Implementa4:1MUXandwritethetestbenchcodetoverifythemodule: Multiplexer (4:1) Verilog design:  module mux41(  input i0,i1,i2,i3,sel0,sel1, output reg y); always @(\*) begin  case ({sel0,sel1}) 2'b00 : y = i0; 2'b01 : y = i1; 2'b10 : y = i2; 2'b11 : y = i3; end case end  endmodul  e  Test Bench:  module tb\_mux41;  reg I0,I1,I2,I3,SEL0,SEL1; wire Y; mux41 MUX (.i0(I0),.i1(I1),.i2(I2),.i3(I3),.sel0(SEL0),.sel1(SEL1),.y(Y)); initial begin I0 =1'b0; I1= 1'b0; I2 =1'b0;  I3 =1'b0; SEL0 =1'b0; SEL1 =1'b0; #45 $finish; end  always #2 I0 = ~I0; always #4 I1 =~I1; always #6 I2 =~I1; always #8 I3 =~I1; always #3 SEL0 = ~SEL0; always #  SEL1 = ~SEL1; always @(Y) |

3